Modeling Methodology for Sequoia India Investment Memo

Energy Innovation modeled Sequioa Climate Foundation’s (SCF) India investments using version 3.1.3 of the Energy Policy Simulator (EPS), an open-source systems dynamics model that simulates the impact of energy and climate policies on greenhouse gas emissions, energy use, and other economic and social indicators. Compared with a business-as-usual scenario, Energy Innovation’s modeled EPS policy scenario estimates 87 MMT CO2e avoided in 2030, and a cumulative 5.5 GT CO2e avoided between now and 2050. The largest savings are in the industry sector followed by the electricity sector and buildings.

The following table summarizes the policies or intended policy impacts of SCF’s India investment portfolio. The sections following the table provide more detail on the key assumptions and methodology for modeling each sector’s policies.

|  |  |
| --- | --- |
| **Electricity Sector Policy** | **Description** |
| Increase in non-fossil fuel capacity | Between 2024 and 2026, India adds 90 GW of non-fossil fuel capacity resulting in 30 percent non-fossil fuel electricity generation. |
| Replace coal capacity with flexible demand | Starting in 2024, India achieves 5 GW of flexible resource by 2026 and 10 GW by 2030. |
| **Industry Sector Policy** | **Description** |
| Phase down HFCs | India ratifies and meets the Kigali Amendment. |
| Reduce electricity demand relative to BAU | Every year between 2026 and 2030, there is an additional 2-3% reduction in total industrial electricity demand compared to BAU electricity demand in that year. |
| **Buildings Sector Policy** | **Description** |
| Reduce electricity demand relative to BAU | Every year between 2026 and 2030, there is an additional 2-3% reduction in total buildings electricity demand compared to BAU electricity demand in that year. |

## Electricity Sector

### Increase in non-fossil fuel capacity

In the EPS, the clean electricity standard policy lever stimulates renewable capacity additions and additional renewable electricity generation. The share of generation from non-fossil fuel sources (renewables plus nuclear) in the EPS BAU is already 37%, and the share of generation from renewables (hydropower, solar, wind, biomass, and geothermal) is 32%.

### Replace coal capacity with flexible demand

In the EPS, we use the demand response policy lever to achieve 8% of demand response potential in 2026 and 11% of the potential in 2030. These settings correspond to 5 GW of demand response and 10 GW in 2030, respectively. In our policy scenario, we assume that each unit of demand response corresponds with an equivalent capacity reduction in coal power generation.[[1]](#footnote-1) To achieve 10 GW of coal reduction in 2030 in our policy scenario compared with the BAU, we also use the early retirement lever in the EPS to retire 1.6 GW of coal in 2030.

## Industry Sector

### Phase down HFCs

We referenced Velders et al. (2022)[[2]](#footnote-2) to estimate the impact of the Kigali Amendment on India’s emissions. We calculated the average reductions in Velders et al.’s KA-2022 scenario and turned on the various f-gas reduction policy levers in the EPS to meet these targeted reductions.

### Reduce electricity demand relative to BAU

The targeted improvement in energy efficiency in every year between 2026 and 2030 is 2-3%, with the average improvement being 2.5%. We use the average to calculate the targeted cumulative percentage improvement in total industrial electricity demand with respect to the BAU in each year. The industry energy efficiency standards policy lever in the EPS is turned on for electricity across the chemicals, agriculture, and “other industries” subsectors to achieve the targeted efficiency improvements.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Cumulative % electricity demand reduction vs BAU** | **2026** | **2027** | **2028** | **2029** | **2030** |
| Low | 2% | 4% | 6% | 8% | 10% |
| High | 3% | 6% | 9% | 12% | 15% |
| Average | 2.5% | 5.0% | 7.5% | 10.0% | 12.5% |

## Buildings Sector

### Reduce electricity demand relative to BAU

The targeted improvement in energy efficiency in every year between 2026 and 2030 is 2-3%, with the average improvement being 2.5%. Similar to the approach for the industry efficiency objective, we use the average to calculate the targeted cumulative percentage improvement in total buildings electricity demand with respect to the BAU in each year. The building energy efficiency standards policy lever in the EPS is turned on for the cooling and ventilation, lighting, appliances, and “other components” categories across all building types (urban residential, rural residential, commercial) to achieve the targeted efficiency improvements.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Cumulative % electricity demand reduction vs BAU** | **2026** | **2027** | **2028** | **2029** | **2030** |
| Low | 2% | 4% | 6% | 8% | 10% |
| High | 3% | 6% | 9% | 12% | 15% |
| Average | 2.5% | 5.0% | 7.5% | 10.0% | 12.5% |

## Additional Information

### Macroeconomic impacts

Our modeled policy scenario does not include any policies to make up for lost government revenue from fossil fuels. From 2024 to 2050, the projected cumulative total loss in government revenue resulting from the policy scenario amounts to $45 billion 2012 US dollars.

### Supporting information

Additional supporting information including workbooks with calculations are available in the “Calculations and Notes” subfolder of the of the SCF\_India\_Analysis branch of Energy Innovation's eps-india GitHub repository.

1. Based on the 2017 LBNL study that Sequoia shared with Energy Innovation. See supporting information. [↑](#footnote-ref-1)
2. See supporting information. [↑](#footnote-ref-2)